Check before starting a print:

1. Enough filament left?
2. Extruder tension bolt tightened?
3. Bed surface clean including wipe area?
4. Bed glue in good shape?